# Open_Adv_Flow_From_Temperature

Syntax

  Bc Flux For Cvfem_Energy [{of} SpeciesName | {in} MaterialPhaseName | {ls} {a | b | c}] {on} Mesh Extent Name [Touching TouchingMeshExtent | Opposing OpposingMeshExtent] = Open_Adv_Flow_From_Temperature [Using Data Specification Data Spec Name] [Data = data | Temperature = temperature | Pressure = pressure | Mass_Fraction_0 = mass_fraction_0 | Mass_Fraction_1 = mass_fraction_1 | Mass_Fraction_2 = mass_fraction_2 | Mass_Fraction_3 = mass_fraction_3 | Mass_Fraction_4 = mass_fraction_4 | Mass_Fraction_5 = mass_fraction_5 | Mass_Fraction_6 = mass_fraction_6 | Mass_Fraction_7 = mass_fraction_7 | Mass_Fraction_8 = mass_fraction_8 | Total_Pressure = total_pressure]

Summary

  CVFEM energy open advective flow from temperature flux

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
{on} | {@ | at | for | in | on | over} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
data | “string” | –
temperature | real | 0
pressure | real | 0
mass_fraction_0 | real | 0
mass_fraction_1 | real | 0
mass_fraction_2 | real | 0
mass_fraction_3 | real | 0
mass_fraction_4 | real | 0
mass_fraction_5 | real | 0
mass_fraction_6 | real | 0
mass_fraction_7 | real | 0
mass_fraction_8 | real | 0
total_pressure | real | 0