# Kinematic

Syntax

  Bc Rotated For Cvfem_Mesh ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} Mesh Extent Name ([Touching TouchingMeshExtent] | [Opposing OpposingMeshExtent]) = Kinematic [Using Data Specification Data Spec Name] ([Unrotated = unrotated] | [V0 = v0] | [Shared_Normal = shared_normal] | [No_Mesh_Movement = no_mesh_movement])

Summary

  Kinematic model for rotated CVFEM_MESH boundary condition

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
unrotated | “string” | –
v0 | real | 0
shared_normal | “string” | –
no_mesh_movement | “string” | –