# Porous_Fluid_Coupling_With_Solid_Convection

Syntax

  Bc Interface For Cvfem_Energy ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} Mesh Extent Name ([Touching TouchingMeshExtent] | [Opposing OpposingMeshExtent]) = Porous_Fluid_Coupling_With_Solid_Convection [Using Data Specification Data Spec Name] ([Toggle = toggle] | [Coeff_Scaling = coeff_scaling] | [Scale_Factor = scale_factor] | [Include_Average_Pressure = include_average_pressure] | [Multiplier = multiplier])

Summary

  Interface BC for porous fluid coupling

Description

  The following options are present in most boundary conditions/sources. The meaning of each option is as follows:

  Toggle

    If given, specifies which toggle block controls whether this BC is active or not.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
toggle | “string” | –
coeff_scaling | real | 1
scale_factor | real | 1
include_average_pressure | integer | 0
multiplier | real | 1