# Open_Adv_Flow

Syntax

  Bc Lumped_Flux For Cvfem_Momentum ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} Mesh Extent Name ([Touching TouchingMeshExtent] | [Opposing OpposingMeshExtent]) = Open_Adv_Flow [Using Data Specification Data Spec Name] ([Pressure = pressure] | [Total_Pressure = total_pressure] | [Coflow_Entrainment_Value_X = coflow_entrainment_value_x] | [Coflow_Entrainment_Value_Y = coflow_entrainment_value_y] | [Coflow_Entrainment_Value_Z = coflow_entrainment_value_z])

Summary

  CVFEM momentum open advective flow flux BC

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
pressure | real | 0
total_pressure | real | 0
coflow_entrainment_value_x | real | 0
coflow_entrainment_value_y | real | 0
coflow_entrainment_value_z | real | 0