# Conductance

Syntax

  Bc Bulknode_Flux For Cvfem_Energy ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} Mesh Extent Name ([Touching TouchingMeshExtent] | [Opposing OpposingMeshExtent]) = Conductance [Using Data Specification Data Spec Name] ([Bulk_Node = bulk_node] | [Toggle = toggle])

Summary

  Applies a contact heat flux of the form to sides and of the contact interface where is a user specified conductance coefficient. Used in conjunction with a CONDUCTANCE COEFFICIENT model.

Description

  The following options are present in most boundary conditions/sources. The meaning of each option is as follows:

  Toggle

    If given, specifies which toggle block controls whether this BC is active or not.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
bulk_node | “string” | –
toggle | “string” | –