# Mass_Flux_From_Temperature

Syntax

  Bc Lumped_Flux For Cvfem_Energy ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} Mesh Extent Name ([Touching TouchingMeshExtent] | [Opposing OpposingMeshExtent]) = Mass_Flux_From_Temperature ([Data = data] | [Temperature = temperature] | [Pressure = pressure] | [Mass_Fraction_0 = mass_fraction_0] | [Mass_Fraction_1 = mass_fraction_1] | [Mass_Fraction_2 = mass_fraction_2] | [Mass_Fraction_3 = mass_fraction_3] | [Mass_Fraction_4 = mass_fraction_4] | [Mass_Fraction_5 = mass_fraction_5] | [Mass_Fraction_6 = mass_fraction_6] | [Mass_Fraction_7 = mass_fraction_7] | [Mass_Fraction_8 = mass_fraction_8] | Total_Mdot = total_mdot)

Summary

  CVFEM energy mass flux from temperature flux BC

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
data | “string” | –
temperature | real | 0
pressure | real | 0
mass_fraction_0 | real | 0
mass_fraction_1 | real | 0
mass_fraction_2 | real | 0
mass_fraction_3 | real | 0
mass_fraction_4 | real | 0
mass_fraction_5 | real | 0
mass_fraction_6 | real | 0
mass_fraction_7 | real | 0
mass_fraction_8 | real | 0
total_mdot | real | –