This section is referenced in the following other sections

- Simulation Setup: Composite

# 7.12.10. Composite Boundary Condition On Surface

Scope

  Fuego Region

Summary

  Defines a thermally-decomposing composite material wall boundary condition that outgasses flammable species when heated sufficiently.

    begin Composite Boundary Condition On Surface Surfacename

        {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} Value

       Activate Backside Convection

       Activate Backside Radiation

       Activate Particle Deposition

       Calculate Convection Coefficient Using Tref {=} Tref ([Dt_Min {=} DTmin]  | [{clip}])

       Composite {backside_convection_coefficient | backside_reference_temperature | initial_temperature | max_nonlinear_iterations | max_thickness | min_nonlinear_iterations | nodes | residual_tolerance | subcycle_safety_factor | thickness} {=} value

       Composite Initial_Mass_Fraction Species {=} value

       Composite Material {=} material_name

       Emissivity Spectral File Name {=} Name

       External Field For VariableName [{of} Species] {=} ExtFieldName [ Of Size Value With Multiplier {=} Multiplier  ]

       External Field For Composite {backside_convection_coefficient | backside_reference_temperature | initial_temperature | max_nonlinear_iterations | max_thickness | min_nonlinear_iterations | nodes | residual_tolerance | subcycle_safety_factor | thickness} {=} ExtFieldName

       Emissivity {=} value

       Function For {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} FuncName [ In The {t | x | y | z} Direction  ]

       Function For Composite {backside_convection_coefficient | backside_reference_temperature | initial_temperature | max_nonlinear_iterations | max_thickness | min_nonlinear_iterations | nodes | residual_tolerance | subcycle_safety_factor | thickness} {=} functionName [ In The {t | x | y | z} Direction  ]

       Function For Composite Initial_Mass_Fraction {=} funcName In The {t | x | y | z} Direction

       Function For Emissivity {=} functionName [ In The {t | x | y | z} Direction  ]

       Function For Mass_Fraction {=} FuncName In The {t | x | y | z} Direction

       Function For Mole_Fraction {=} FuncName In The {t | x | y | z} Direction

       Function For Radiation Boundary Temperature {=} functionName

       Function For Radiation Environment Temperature {=} functionName

       Function For Transmissivity {=} functionName [ In The {t | x | y | z} Direction  ]

       Function For Transparent Band Emissivity {=} functionName [ In The {t | x | y | z} Direction  ]

       Function For Wall Temperature {=} functionName [ In The {t | x | y | z} Direction  ]

       Inline Function For {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} FuncStr

       Integer Data For Subroutine SubName {=} Values...

       Interface Boundary

       Mass_Fraction Species {=} Mass fraction

       Mole_Fraction Species {=} Mole fraction

       Particle Species {=} species_name...

       Post Process Yplus

       Postprocess FluxType Flux Of {conserved_enthalpy | continuity | edc_product | enthalpy | mixture_fraction | nuclei | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot | species | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_momentum | x_solid_momentum | y_momentum | y_solid_momentum | z_momentum | z_solid_momentum} [ As aliases...  ]

       Project Nodes

       Progress_Variable ProgressVariableName {=} Value

       Real Data For Subroutine SubName {=} Values...

       Radiation Boundary Temperature {=} value

       Radiation Boundary Temperature Field {=} FieldName

       Radiation Environment Temperature {=} value

       Radiation Environment Temperature Field {=} FieldName

       Subroutine For {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} Subroutine

       Subroutine For Composite {backside_convection_coefficient | backside_reference_temperature | initial_temperature | max_nonlinear_iterations | max_thickness | min_nonlinear_iterations | nodes | residual_tolerance | subcycle_safety_factor | thickness} {=} subroutineName

       Subroutine For Emissivity {=} subroutineName

       Subroutine For Mass_Fraction {=} Subroutine

       Subroutine For Mole_Fraction {=} Subroutine

       Subroutine For Radiation Boundary Temperature {=} subroutineName

       Subroutine For Radiation Environment Temperature {=} subroutineName

       Subroutine For Transmissivity {=} subroutineName

       Subroutine For Transparent Band Emissivity {=} subroutineName

       Subroutine For Wall Temperature {=} subroutineName

       Transparent Band Emissivity {=} value

       Transmissivity {=} value

       Use Equilibrium Production Model

       Wall Temperature {=} value

       Law_Of_Wall_Roughness_Parameter {=} Law of the Wall Roughness parameter

    end Composite Boundary Condition On Surface Surfacename

## 7.12.10.1. Line Commands

###### Primitivevariable

Syntax

  Primitivevariable {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} Value

Summary

  Value for the specified variable (in consistent units). Value can be a constant or a string function of position (x,y,z), time (t), and any global variable.

  The function string must be enclosed in quotes if it has spaces or commas. For example: x_velocity = “min(1, 0.1*t)”

Parameter | Value | Default
--- | --- | ---
PrimitiveVariable | {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} | –
{=} | {= | are | is} | –
Value | “string” | –

###### Activate Backside Convection

Syntax

  Activate Backside Convection

Summary

  Turn on model for convective heat transfer on the back side of the composite material. A convection coefficient and reference temperature must also be specified.

###### Activate Backside Radiation

Syntax

  Activate Backside Radiation

Summary

  Turn on model for radiative heat transfer on the back side of the composite material. A reference temperature must also be specified.

###### Activate Particle Deposition

Syntax

  Activate Particle Deposition

Summary

  Turn on deposition of material from the accumulation of particles on the composite material. A species name for the particles must also be supplied. Currently only one species is supported.

###### Calculate Convection Coefficient

Syntax

  Calculate Convection Coefficient Using Tref {=} Tref ([Dt_Min {=} DTmin] | [{clip}])

Summary

  Calculates the convection coefficient on the wall using a user-specified value for the reference temperature. This calculates .

  > can be a constant, or a string function of time and global variables.

  > By default, is set to 0 if however a different tolerance can be supplied with .

  > The optional ‘clip’ argument will clip the calculated value of to be non-negative.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
Tref | “string” | –
{=} | {= | are | is} | –
DTmin | real | –
Clip | {clip} | –

###### Composite

Syntax

  Composite {backside_convection_coefficient | backside_reference_temperature | initial_temperature | max_nonlinear_iterations | max_thickness | min_nonlinear_iterations | nodes | residual_tolerance | subcycle_safety_factor | thickness} {=} value

Summary

  Parameters for composite fire model.

Parameter | Value | Default
--- | --- | ---
CompositeVariable | {backside_convection_coefficient | backside_reference_temperature | initial_temperature | max_nonlinear_iterations | max_thickness | min_nonlinear_iterations | nodes | residual_tolerance | subcycle_safety_factor | thickness} | –
{=} | {= | are | is} | –
value | real | –

###### Composite Initial_Mass_Fraction

Syntax

  Composite Initial_Mass_Fraction Species {=} value

Summary

  Constant value for the initial mass fraction of selected species in the composite.

Parameter | Value | Default
--- | --- | ---
Species | string | –
{=} | {= | are | is} | –
value | “string” | –

###### Composite Material

Syntax

  Composite Material {=} material_name

Summary

  Name of the Fuego material to use for the composite BC.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
material_name | string | –

###### Emissivity Spectral File Name

Syntax

  Emissivity Spectral File Name {=} Name

Summary

  Specify the file name for defining spectral radiation properties on a surface.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
Name | string | –

###### External Field For

Syntax

  External Field For VariableName [{of} Species] {=} ExtFieldName [ Of Size Value With Multiplier {=} Multiplier ]

Summary

  Name of the field that is to be transferred in. For species equation, specify variable as “mass fraction of” followed by the species name for transfers associated with separated individual species field names.

Parameter | Value | Default
--- | --- | ---
VariableName | string | –
Species | string | –
{=} | {= | are | is} | –
ExtFieldName | string | –

###### External Field For Composite

Syntax

  External Field For Composite {backside_convection_coefficient | backside_reference_temperature | initial_temperature | max_nonlinear_iterations | max_thickness | min_nonlinear_iterations | nodes | residual_tolerance | subcycle_safety_factor | thickness} {=} ExtFieldName

Summary

  Name of an external field to use for composite variable.

Parameter | Value | Default
--- | --- | ---
CompositeVariable | {backside_convection_coefficient | backside_reference_temperature | initial_temperature | max_nonlinear_iterations | max_thickness | min_nonlinear_iterations | nodes | residual_tolerance | subcycle_safety_factor | thickness} | –
{=} | {= | are | is} | –
ExtFieldName | string | –

###### Emissivity

Syntax

  Emissivity {=} value

Summary

  Constant value for emissivity variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
value | “string” | –

###### Function For

Syntax

  Function For {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} FuncName [ In The {t | x | y | z} Direction ]

Summary

  Name of function to use for the given variable, in the specified direction.

Parameter | Value | Default
--- | --- | ---
PrimitiveVariable | {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} | –
{=} | {= | are | is} | –
FuncName | string | –

###### Function For Composite

Syntax

  Function For Composite {backside_convection_coefficient | backside_reference_temperature | initial_temperature | max_nonlinear_iterations | max_thickness | min_nonlinear_iterations | nodes | residual_tolerance | subcycle_safety_factor | thickness} {=} functionName [ In The {t | x | y | z} Direction ]

Summary

  Name of function to use for the given composite fire variable, in the specified direction.

Parameter | Value | Default
--- | --- | ---
CompositeVariable | {backside_convection_coefficient | backside_reference_temperature | initial_temperature | max_nonlinear_iterations | max_thickness | min_nonlinear_iterations | nodes | residual_tolerance | subcycle_safety_factor | thickness} | –
{=} | {= | are | is} | –
functionName | string | –

###### Function For Composite Initial_Mass_Fraction

Syntax

  Function For Composite Initial_Mass_Fraction {=} funcName In The {t | x | y | z} Direction

Summary

  Name of the mass fraction function to use for all species in the composite in a given direction. Note that this must be a Multicolumn function

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
funcName | string | –
Direction | {t | x | y | z} | –

###### Function For Emissivity

Syntax

  Function For Emissivity {=} functionName [ In The {t | x | y | z} Direction ]

Summary

  Name of the function to use for the emissivity in the given direction (default direction = time).

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
functionName | string | –

###### Function For Mass_Fraction

Syntax

  Function For Mass_Fraction {=} FuncName In The {t | x | y | z} Direction

Summary

  Name of the mass fraction function to use for all species in the given direction. Note that this must be a Multicolumn function

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
FuncName | string | –
Direction | {t | x | y | z} | –

###### Function For Mole_Fraction

Syntax

  Function For Mole_Fraction {=} FuncName In The {t | x | y | z} Direction

Summary

  Name of the mass fraction function to use for all species in the given direction. Note that this must be a Multicolumn function

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
FuncName | string | –
Direction | {t | x | y | z} | –

###### Function For Radiation Boundary Temperature

Syntax

  Function For Radiation Boundary Temperature {=} functionName

Summary

  Name of function to use for the radiation_boundary_temperature variable

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
functionName | string | –

###### Function For Radiation Environment Temperature

Syntax

  Function For Radiation Environment Temperature {=} functionName

Summary

  Name of function to use for the radiation_environment_temperature variable

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
functionName | string | –

###### Function For Transmissivity

Syntax

  Function For Transmissivity {=} functionName [ In The {t | x | y | z} Direction ]

Summary

  Name of function to use for the transmissivity variable

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
functionName | string | –

###### Function For Transparent Band Emissivity

Syntax

  Function For Transparent Band Emissivity {=} functionName [ In The {t | x | y | z} Direction ]

Summary

  Name of function to use for the transparent emissivity band for spectral emissivity on surfaces.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
functionName | string | –

###### Function For Wall Temperature

Syntax

  Function For Wall Temperature {=} functionName [ In The {t | x | y | z} Direction ]

Summary

  Name of function to use for the wall_temperature variable, in the specified direction.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
functionName | string | –

###### Inline Function For

Syntax

  Inline Function For {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} FuncStr

Summary

  warning{This command is deprecated. Regular BCs now support using string functions directly}

Parameter | Value | Default
--- | --- | ---
PrimitiveVariable | {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} | –
{=} | {= | are | is} | –
FuncStr | “string” | –

###### Integer Data For Subroutine

Syntax

  Integer Data For Subroutine SubName {=} Values…

Summary

  List of integer data values to be passed down in to the user subroutine. These values may be changed by the user subroutine.

Parameter | Value | Default
--- | --- | ---
SubName | string | –
{=} | {= | are | is} | –
Values | integer… | –

###### Interface Boundary

Syntax

  Interface Boundary

Summary

  Mark this fluids boundary as an interface between two physical regions. Data will be interpolated across this boundary.

###### Mass_Fraction

Syntax

  Mass_Fraction Species {=} Mass fraction

Summary

  Value for the mass fraction of selected species. Can be a constant value or a string function of space (x,y,z), time (t), and any global variable.

Parameter | Value | Default
--- | --- | ---
Species | string | –
{=} | {= | are | is} | –
Mass fraction | “string” | –

###### Mole_Fraction

Syntax

  Mole_Fraction Species {=} Mole fraction

Summary

  Value for the mole fraction of selected species. Can be a constant value or a string function of space (x,y,z), time (t), and any global variable.

Parameter | Value | Default
--- | --- | ---
Species | string | –
{=} | {= | are | is} | –
Mole fraction | “string” | –

###### Particle Species

Syntax

  Particle Species {=} species_name…

Summary

  Names of the particle species that can accumulate on the composite BC (this must be the complete list of species in the particle definition, listed in the same order as defined in the particle definition).

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
species_name | string… | –

###### Post Process Yplus

Syntax

  Post Process Yplus

Summary

  Request post processing of yplus on this mesh part.

Description

  The normalized distance to the wall () can be post-processed on any wall (laminar or turbulent). Yplus is calculated in a manner consistent with how it is calculated in the solution procedure. Max/min values are provided as output at every wall. This option computes and stores the entire field along the wall. Since this option computes using the most recent values for all solution variables, the max/min written to the log may differ from the max/min of this field. However, these will become identical at convergence.

  Note that this line command does not automatically output this field to a results file. For that, one must use the standard output line command for a nodal field using the string name, `yplus`.

###### Postprocess

Syntax

  Postprocess FluxType Flux Of {conserved_enthalpy | continuity | edc_product | enthalpy | mixture_fraction | nuclei | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot | species | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_momentum | x_solid_momentum | y_momentum | y_solid_momentum | z_momentum | z_solid_momentum} [ As aliases… ]

Summary

  Enable nodal flux post-processing for a given equation. Flux types can be “total”, “advective”, or “diffusive”. Integrated fluxes will also be output to global variables for post-processing or use in other string functions.

  By default the variables will be named based on the equation and sideset they are applied to as bc_FluxType_EquationName_flux_SurfaceName. However, if you want to assign a more compact or descriptive name you can provide it with

      POSTPROCESS TOTAL FLUX OF Continuity AS mdot1

  When post-processing enthalpy, the average temperature is also output as a global variable. If you provide only one alias the enthalpy flux uses your alias and the average temperature is automatically named. If you provide two aliases the first is used for enthalpy and the second is used for temperature.

      POSTPROCESS TOTAL FLUX OF ENTHALPY AS hFlux
      POSTPROCESS TOTAL FLUX OF ENTHALPY AS hFlux Tavg

  When post-processing species, the post-processor is run for each species that is solved for. This means that there is no post-processor run on the last species (which is determined by a fractional balance). If you provide aliases for the species post-processor you should provide one for each post-processed species. For example, in a problem with O2, CO2, and N2 (in that order) you could use:

      POSTPROCESS TOTAL FLUX OF SPECIES AS mdotO2 mdotCO2

Parameter | Value | Default
--- | --- | ---
FluxType | string | –
equation | {conserved_enthalpy | continuity | edc_product | enthalpy | mixture_fraction | nuclei | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot | species | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_momentum | x_solid_momentum | y_momentum | y_solid_momentum | z_momentum | z_solid_momentum} | –

###### Project Nodes

Syntax

  Project Nodes

Summary

  Allow for nodal projection on the particular mesh part.

Description

  The nodal projection of velocity is defaulted to occur on open boundary conditions only. Wall and inflow BCs are defaulted to not be projected, even on flux inflow (i.e., `USE FLUXES`) and turbulent wall nodes. This option flags the particular mesh part to be included in the nodes to be projected.

###### Progress_Variable

Syntax

  Progress_Variable ProgressVariableName {=} Value

Summary

  Constant value for the progress variable of selected scalars.

Parameter | Value | Default
--- | --- | ---
ProgressVariableName | string | –
{=} | {= | are | is} | –
Value | real | –

###### Real Data For Subroutine

Syntax

  Real Data For Subroutine SubName {=} Values…

Summary

  List of real data values to be passed down in to the user subroutine. These values may be changed by the user subroutine.

Parameter | Value | Default
--- | --- | ---
SubName | string | –
{=} | {= | are | is} | –
Values | real… | –

###### Radiation Boundary Temperature

Syntax

  Radiation Boundary Temperature {=} value

Summary

  Constant value for radiation_boundary_temperature variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
value | “string” | –

###### Radiation Boundary Temperature Field

Syntax

  Radiation Boundary Temperature Field {=} FieldName

Summary

  Name of the field to use for the radiation boundary temperature.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
FieldName | string | –

###### Radiation Environment Temperature

Syntax

  Radiation Environment Temperature {=} value

Summary

  Constant value for radiation_environment_temperature variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
value | “string” | –

###### Radiation Environment Temperature Field

Syntax

  Radiation Environment Temperature Field {=} FieldName

Summary

  Name of the field to use for the radiation environment temperature.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
FieldName | string | –

###### Subroutine For

Syntax

  Subroutine For {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} Subroutine

Summary

  Name of the subroutine to use for this variable.

Parameter | Value | Default
--- | --- | ---
PrimitiveVariable | {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} | –
{=} | {= | are | is} | –
Subroutine | string | –

###### Subroutine For Composite

Syntax

  Subroutine For Composite {backside_convection_coefficient | backside_reference_temperature | initial_temperature | max_nonlinear_iterations | max_thickness | min_nonlinear_iterations | nodes | residual_tolerance | subcycle_safety_factor | thickness} {=} subroutineName

Summary

  Name of the user subroutine to use for the given composite fire variable.

Parameter | Value | Default
--- | --- | ---
CompositeVariable | {backside_convection_coefficient | backside_reference_temperature | initial_temperature | max_nonlinear_iterations | max_thickness | min_nonlinear_iterations | nodes | residual_tolerance | subcycle_safety_factor | thickness} | –
{=} | {= | are | is} | –
subroutineName | string | –

###### Subroutine For Emissivity

Syntax

  Subroutine For Emissivity {=} subroutineName

Summary

  Name of the user subroutine to use for the emissivity variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subroutineName | string | –

###### Subroutine For Mass_Fraction

Syntax

  Subroutine For Mass_Fraction {=} Subroutine

Summary

  Name of the subroutine to use for the mass fraction. ALL species mass fractions must be assigned by this subroutine.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
Subroutine | string | –

###### Subroutine For Mole_Fraction

Syntax

  Subroutine For Mole_Fraction {=} Subroutine

Summary

  Name of the subroutine to use for the mole fractions. ALL species mole fractions must be assigned by this subroutine.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
Subroutine | string | –

###### Subroutine For Radiation Boundary Temperature

Syntax

  Subroutine For Radiation Boundary Temperature {=} subroutineName

Summary

  Name of the user subroutine to use for the radiation_boundary_temperature variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subroutineName | string | –

###### Subroutine For Radiation Environment Temperature

Syntax

  Subroutine For Radiation Environment Temperature {=} subroutineName

Summary

  Name of the user subroutine to use for the radiation_environment_temperature variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subroutineName | string | –

###### Subroutine For Transmissivity

Syntax

  Subroutine For Transmissivity {=} subroutineName

Summary

  Name of the user subroutine to use for the transmissivity variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subroutineName | string | –

###### Subroutine For Transparent Band Emissivity

Syntax

  Subroutine For Transparent Band Emissivity {=} subroutineName

Summary

  Name of the user subroutine to use for the transparent emissivity band for spectral emissivity on surfaces.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subroutineName | string | –

###### Subroutine For Wall Temperature

Syntax

  Subroutine For Wall Temperature {=} subroutineName

Summary

  Name of the user subroutine to use for the wall_temperature variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subroutineName | string | –

###### Transparent Band Emissivity

Syntax

  Transparent Band Emissivity {=} value

Summary

  Constant value to use for the emissivity in the transparent band for spectral surfaces.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
value | “string” | –

###### Transmissivity

Syntax

  Transmissivity {=} value

Summary

  Constant value for transmissivity variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
value | “string” | –

###### Use Equilibrium Production Model

Syntax

  Use Equilibrium Production Model

Summary

  Change near-wall turbulence production.

Description

  This option specifies that the near wall turb_ke production term is given by:

  . Modifications are made for the KW and SST model. This model is suggested when using the standard KW and SST model when a Dirichlet condition is not placed on the wall node of turbulence kinetic energy.

###### Wall Temperature

Syntax

  Wall Temperature {=} value

Summary

  Value for wall_temperature variable. Can be a constant or a string function of space (x,y,z), time (t) or global variables.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
value | “string” | –

###### Law_Of_Wall_Roughness_Parameter

Syntax

  Law_Of_Wall_Roughness_Parameter {=} Law of the Wall Roughness parameter

Summary

  Specify dimensionless roughness factor to be used in the law-of-the-wall formulation.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
Law of the Wall Roughness parameter | real | 9.8

# 7.12.11. Composite Interface Boundary Condition On Surface

Scope

  Fuego Region

Summary

  Defines a wall interface boundary condition that outgasses flammable species when heated sufficiently. This boundary condition may be treated as a porous composite material wall where the heat flux, mass transfer and pressure are applied from a coupled region via a transfer. This boundary enforces Dirichlet-Robin coupling.

  Sign Convention: If transferring a field for composite_mass_rate or composite_species_mass_rate, the expected sign convention is positive for flows into the Fuego domain. If the transferred field has the opposite convention use the multiplier option with a value of -1.

    begin Composite Interface Boundary Condition On Surface Surfacename

        {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} Value

       Calculate Convection Coefficient Using Tref {=} Tref ([Dt_Min {=} DTmin]  | [{clip}])

       Composite Initial_Mass_Fraction Species {=} value

       Emissivity Spectral File Name {=} Name

       External Field For VariableName [{of} Species] {=} ExtFieldName [ Of Size Value With Multiplier {=} Multiplier  ]

       Emissivity {=} value

       Function For {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} FuncName [ In The {t | x | y | z} Direction  ]

       Function For Composite Initial_Mass_Fraction {=} funcName In The {t | x | y | z} Direction

       Function For Emissivity {=} functionName [ In The {t | x | y | z} Direction  ]

       Function For Mass_Fraction {=} FuncName In The {t | x | y | z} Direction

       Function For Mole_Fraction {=} FuncName In The {t | x | y | z} Direction

       Function For Radiation Boundary Temperature {=} functionName

       Function For Radiation Environment Temperature {=} functionName

       Function For Transmissivity {=} functionName [ In The {t | x | y | z} Direction  ]

       Function For Transparent Band Emissivity {=} functionName [ In The {t | x | y | z} Direction  ]

       Function For Wall Temperature {=} functionName [ In The {t | x | y | z} Direction  ]

       Inline Function For {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} FuncStr

       Integer Data For Subroutine SubName {=} Values...

       Interface Boundary

       Mass_Fraction Species {=} Mass fraction

       Mole_Fraction Species {=} Mole fraction

       Post Process Yplus

       Postprocess FluxType Flux Of {conserved_enthalpy | continuity | edc_product | enthalpy | mixture_fraction | nuclei | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot | species | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_momentum | x_solid_momentum | y_momentum | y_solid_momentum | z_momentum | z_solid_momentum} [ As aliases...  ]

       Project Nodes

       Progress_Variable ProgressVariableName {=} Value

       Real Data For Subroutine SubName {=} Values...

       Radiation Boundary Temperature {=} value

       Radiation Boundary Temperature Field {=} FieldName

       Radiation Environment Temperature {=} value

       Radiation Environment Temperature Field {=} FieldName

       Subroutine For {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} Subroutine

       Subroutine For Composite Initial_Mass_Fraction {=} subName

       Subroutine For Emissivity {=} subroutineName

       Subroutine For Mass_Fraction {=} Subroutine

       Subroutine For Mole_Fraction {=} Subroutine

       Subroutine For Radiation Boundary Temperature {=} subroutineName

       Subroutine For Radiation Environment Temperature {=} subroutineName

       Subroutine For Transmissivity {=} subroutineName

       Subroutine For Transparent Band Emissivity {=} subroutineName

       Subroutine For Wall Temperature {=} subroutineName

       Transparent Band Emissivity {=} value

       Transmissivity {=} value

       Use Equilibrium Production Model

       Wall Temperature {=} value

       Law_Of_Wall_Roughness_Parameter {=} Law of the Wall Roughness parameter

    end Composite Interface Boundary Condition On Surface Surfacename

## 7.12.11.1. Line Commands

###### Primitivevariable

Syntax

  Primitivevariable {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} Value

Summary

  Value for the specified variable (in consistent units). Value can be a constant or a string function of position (x,y,z), time (t), and any global variable.

  The function string must be enclosed in quotes if it has spaces or commas. For example: x_velocity = “min(1, 0.1*t)”

Parameter | Value | Default
--- | --- | ---
PrimitiveVariable | {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} | –
{=} | {= | are | is} | –
Value | “string” | –

###### Calculate Convection Coefficient

Syntax

  Calculate Convection Coefficient Using Tref {=} Tref ([Dt_Min {=} DTmin] | [{clip}])

Summary

  Calculates the convection coefficient on the wall using a user-specified value for the reference temperature. This calculates .

  > can be a constant, or a string function of time and global variables.

  > By default, is set to 0 if however a different tolerance can be supplied with .

  > The optional ‘clip’ argument will clip the calculated value of to be non-negative.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
Tref | “string” | –
{=} | {= | are | is} | –
DTmin | real | –
Clip | {clip} | –

###### Composite Initial_Mass_Fraction

Syntax

  Composite Initial_Mass_Fraction Species {=} value

Summary

  Constant value for the initial mass fraction of selected species in the composite.

Parameter | Value | Default
--- | --- | ---
Species | string | –
{=} | {= | are | is} | –
value | “string” | –

###### Emissivity Spectral File Name

Syntax

  Emissivity Spectral File Name {=} Name

Summary

  Specify the file name for defining spectral radiation properties on a surface.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
Name | string | –

###### External Field For

Syntax

  External Field For VariableName [{of} Species] {=} ExtFieldName [ Of Size Value With Multiplier {=} Multiplier ]

Summary

  Name of the field that is to be transferred in. For species equation, specify variable as “mass fraction of” followed by the species name for transfers associated with separated individual species field names.

Parameter | Value | Default
--- | --- | ---
VariableName | string | –
Species | string | –
{=} | {= | are | is} | –
ExtFieldName | string | –

###### Emissivity

Syntax

  Emissivity {=} value

Summary

  Constant value for emissivity variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
value | “string” | –

###### Function For

Syntax

  Function For {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} FuncName [ In The {t | x | y | z} Direction ]

Summary

  Name of function to use for the given variable, in the specified direction.

Parameter | Value | Default
--- | --- | ---
PrimitiveVariable | {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} | –
{=} | {= | are | is} | –
FuncName | string | –

###### Function For Composite Initial_Mass_Fraction

Syntax

  Function For Composite Initial_Mass_Fraction {=} funcName In The {t | x | y | z} Direction

Summary

  Name of the mass fraction function to use for all species in the composite in a given direction. Note that this must be a Multicolumn function

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
funcName | string | –
Direction | {t | x | y | z} | –

###### Function For Emissivity

Syntax

  Function For Emissivity {=} functionName [ In The {t | x | y | z} Direction ]

Summary

  Name of the function to use for the emissivity in the given direction (default direction = time).

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
functionName | string | –

###### Function For Mass_Fraction

Syntax

  Function For Mass_Fraction {=} FuncName In The {t | x | y | z} Direction

Summary

  Name of the mass fraction function to use for all species in the given direction. Note that this must be a Multicolumn function

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
FuncName | string | –
Direction | {t | x | y | z} | –

###### Function For Mole_Fraction

Syntax

  Function For Mole_Fraction {=} FuncName In The {t | x | y | z} Direction

Summary

  Name of the mass fraction function to use for all species in the given direction. Note that this must be a Multicolumn function

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
FuncName | string | –
Direction | {t | x | y | z} | –

###### Function For Radiation Boundary Temperature

Syntax

  Function For Radiation Boundary Temperature {=} functionName

Summary

  Name of function to use for the radiation_boundary_temperature variable

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
functionName | string | –

###### Function For Radiation Environment Temperature

Syntax

  Function For Radiation Environment Temperature {=} functionName

Summary

  Name of function to use for the radiation_environment_temperature variable

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
functionName | string | –

###### Function For Transmissivity

Syntax

  Function For Transmissivity {=} functionName [ In The {t | x | y | z} Direction ]

Summary

  Name of function to use for the transmissivity variable

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
functionName | string | –

###### Function For Transparent Band Emissivity

Syntax

  Function For Transparent Band Emissivity {=} functionName [ In The {t | x | y | z} Direction ]

Summary

  Name of function to use for the transparent emissivity band for spectral emissivity on surfaces.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
functionName | string | –

###### Function For Wall Temperature

Syntax

  Function For Wall Temperature {=} functionName [ In The {t | x | y | z} Direction ]

Summary

  Name of function to use for the wall_temperature variable, in the specified direction.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
functionName | string | –

###### Inline Function For

Syntax

  Inline Function For {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} FuncStr

Summary

  warning{This command is deprecated. Regular BCs now support using string functions directly}

Parameter | Value | Default
--- | --- | ---
PrimitiveVariable | {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} | –
{=} | {= | are | is} | –
FuncStr | “string” | –

###### Integer Data For Subroutine

Syntax

  Integer Data For Subroutine SubName {=} Values…

Summary

  List of integer data values to be passed down in to the user subroutine. These values may be changed by the user subroutine.

Parameter | Value | Default
--- | --- | ---
SubName | string | –
{=} | {= | are | is} | –
Values | integer… | –

###### Interface Boundary

Syntax

  Interface Boundary

Summary

  Mark this fluids boundary as an interface between two physical regions. Data will be interpolated across this boundary.

###### Mass_Fraction

Syntax

  Mass_Fraction Species {=} Mass fraction

Summary

  Value for the mass fraction of selected species. Can be a constant value or a string function of space (x,y,z), time (t), and any global variable.

Parameter | Value | Default
--- | --- | ---
Species | string | –
{=} | {= | are | is} | –
Mass fraction | “string” | –

###### Mole_Fraction

Syntax

  Mole_Fraction Species {=} Mole fraction

Summary

  Value for the mole fraction of selected species. Can be a constant value or a string function of space (x,y,z), time (t), and any global variable.

Parameter | Value | Default
--- | --- | ---
Species | string | –
{=} | {= | are | is} | –
Mole fraction | “string” | –

###### Post Process Yplus

Syntax

  Post Process Yplus

Summary

  Request post processing of yplus on this mesh part.

Description

  The normalized distance to the wall () can be post-processed on any wall (laminar or turbulent). Yplus is calculated in a manner consistent with how it is calculated in the solution procedure. Max/min values are provided as output at every wall. This option computes and stores the entire field along the wall. Since this option computes using the most recent values for all solution variables, the max/min written to the log may differ from the max/min of this field. However, these will become identical at convergence.

  Note that this line command does not automatically output this field to a results file. For that, one must use the standard output line command for a nodal field using the string name, `yplus`.

###### Postprocess

Syntax

  Postprocess FluxType Flux Of {conserved_enthalpy | continuity | edc_product | enthalpy | mixture_fraction | nuclei | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot | species | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_momentum | x_solid_momentum | y_momentum | y_solid_momentum | z_momentum | z_solid_momentum} [ As aliases… ]

Summary

  Enable nodal flux post-processing for a given equation. Flux types can be “total”, “advective”, or “diffusive”. Integrated fluxes will also be output to global variables for post-processing or use in other string functions.

  By default the variables will be named based on the equation and sideset they are applied to as bc_FluxType_EquationName_flux_SurfaceName. However, if you want to assign a more compact or descriptive name you can provide it with

      POSTPROCESS TOTAL FLUX OF Continuity AS mdot1

  When post-processing enthalpy, the average temperature is also output as a global variable. If you provide only one alias the enthalpy flux uses your alias and the average temperature is automatically named. If you provide two aliases the first is used for enthalpy and the second is used for temperature.

      POSTPROCESS TOTAL FLUX OF ENTHALPY AS hFlux
      POSTPROCESS TOTAL FLUX OF ENTHALPY AS hFlux Tavg

  When post-processing species, the post-processor is run for each species that is solved for. This means that there is no post-processor run on the last species (which is determined by a fractional balance). If you provide aliases for the species post-processor you should provide one for each post-processed species. For example, in a problem with O2, CO2, and N2 (in that order) you could use:

      POSTPROCESS TOTAL FLUX OF SPECIES AS mdotO2 mdotCO2

Parameter | Value | Default
--- | --- | ---
FluxType | string | –
equation | {conserved_enthalpy | continuity | edc_product | enthalpy | mixture_fraction | nuclei | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot | species | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_momentum | x_solid_momentum | y_momentum | y_solid_momentum | z_momentum | z_solid_momentum} | –

###### Project Nodes

Syntax

  Project Nodes

Summary

  Allow for nodal projection on the particular mesh part.

Description

  The nodal projection of velocity is defaulted to occur on open boundary conditions only. Wall and inflow BCs are defaulted to not be projected, even on flux inflow (i.e., `USE FLUXES`) and turbulent wall nodes. This option flags the particular mesh part to be included in the nodes to be projected.

###### Progress_Variable

Syntax

  Progress_Variable ProgressVariableName {=} Value

Summary

  Constant value for the progress variable of selected scalars.

Parameter | Value | Default
--- | --- | ---
ProgressVariableName | string | –
{=} | {= | are | is} | –
Value | real | –

###### Real Data For Subroutine

Syntax

  Real Data For Subroutine SubName {=} Values…

Summary

  List of real data values to be passed down in to the user subroutine. These values may be changed by the user subroutine.

Parameter | Value | Default
--- | --- | ---
SubName | string | –
{=} | {= | are | is} | –
Values | real… | –

###### Radiation Boundary Temperature

Syntax

  Radiation Boundary Temperature {=} value

Summary

  Constant value for radiation_boundary_temperature variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
value | “string” | –

###### Radiation Boundary Temperature Field

Syntax

  Radiation Boundary Temperature Field {=} FieldName

Summary

  Name of the field to use for the radiation boundary temperature.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
FieldName | string | –

###### Radiation Environment Temperature

Syntax

  Radiation Environment Temperature {=} value

Summary

  Constant value for radiation_environment_temperature variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
value | “string” | –

###### Radiation Environment Temperature Field

Syntax

  Radiation Environment Temperature Field {=} FieldName

Summary

  Name of the field to use for the radiation environment temperature.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
FieldName | string | –

###### Subroutine For

Syntax

  Subroutine For {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} {=} Subroutine

Summary

  Name of the subroutine to use for this variable.

Parameter | Value | Default
--- | --- | ---
PrimitiveVariable | {contact_angle | edc_product | gas_volume_fraction | mixture_fraction | pressure | progress_variable | scalar_variance | second_mixture_fraction | solid_volume_fraction | soot_mass_fraction | soot_nuclei_mass_fraction | temperature | turbulent_dissipation | turbulent_frequency | turbulent_helmholtz_function | turbulent_kinetic_energy | turbulent_v2 | volume_of_fluid | x_solid_velocity | x_velocity | y_solid_velocity | y_velocity | z_solid_velocity | z_velocity} | –
{=} | {= | are | is} | –
Subroutine | string | –

###### Subroutine For Composite Initial_Mass_Fraction

Syntax

  Subroutine For Composite Initial_Mass_Fraction {=} subName

Summary

  Name of the subroutine to use for the mass fraction. ALL species mass fractions must be assigned by this subroutine.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subName | string | –

###### Subroutine For Emissivity

Syntax

  Subroutine For Emissivity {=} subroutineName

Summary

  Name of the user subroutine to use for the emissivity variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subroutineName | string | –

###### Subroutine For Mass_Fraction

Syntax

  Subroutine For Mass_Fraction {=} Subroutine

Summary

  Name of the subroutine to use for the mass fraction. ALL species mass fractions must be assigned by this subroutine.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
Subroutine | string | –

###### Subroutine For Mole_Fraction

Syntax

  Subroutine For Mole_Fraction {=} Subroutine

Summary

  Name of the subroutine to use for the mole fractions. ALL species mole fractions must be assigned by this subroutine.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
Subroutine | string | –

###### Subroutine For Radiation Boundary Temperature

Syntax

  Subroutine For Radiation Boundary Temperature {=} subroutineName

Summary

  Name of the user subroutine to use for the radiation_boundary_temperature variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subroutineName | string | –

###### Subroutine For Radiation Environment Temperature

Syntax

  Subroutine For Radiation Environment Temperature {=} subroutineName

Summary

  Name of the user subroutine to use for the radiation_environment_temperature variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subroutineName | string | –

###### Subroutine For Transmissivity

Syntax

  Subroutine For Transmissivity {=} subroutineName

Summary

  Name of the user subroutine to use for the transmissivity variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subroutineName | string | –

###### Subroutine For Transparent Band Emissivity

Syntax

  Subroutine For Transparent Band Emissivity {=} subroutineName

Summary

  Name of the user subroutine to use for the transparent emissivity band for spectral emissivity on surfaces.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subroutineName | string | –

###### Subroutine For Wall Temperature

Syntax

  Subroutine For Wall Temperature {=} subroutineName

Summary

  Name of the user subroutine to use for the wall_temperature variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
subroutineName | string | –

###### Transparent Band Emissivity

Syntax

  Transparent Band Emissivity {=} value

Summary

  Constant value to use for the emissivity in the transparent band for spectral surfaces.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
value | “string” | –

###### Transmissivity

Syntax

  Transmissivity {=} value

Summary

  Constant value for transmissivity variable.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
value | “string” | –

###### Use Equilibrium Production Model

Syntax

  Use Equilibrium Production Model

Summary

  Change near-wall turbulence production.

Description

  This option specifies that the near wall turb_ke production term is given by:

  . Modifications are made for the KW and SST model. This model is suggested when using the standard KW and SST model when a Dirichlet condition is not placed on the wall node of turbulence kinetic energy.

###### Wall Temperature

Syntax

  Wall Temperature {=} value

Summary

  Value for wall_temperature variable. Can be a constant or a string function of space (x,y,z), time (t) or global variables.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
value | “string” | –

###### Law_Of_Wall_Roughness_Parameter

Syntax

  Law_Of_Wall_Roughness_Parameter {=} Law of the Wall Roughness parameter

Summary

  Specify dimensionless roughness factor to be used in the law-of-the-wall formulation.

Parameter | Value | Default
--- | --- | ---
{=} | {= | are | is} | –
Law of the Wall Roughness parameter | real | 9.8