GeoTessCPP 2.6.1 Software to facilitate storage and retrieval of 3D information about the Earth.

Loading...
Searching...
No Matches
Class Hierarchy
This inheritance list is sorted roughly, but not completely, alphabetically:
[detail level 1 2]

C geotess::ArrayReuse< T > | An array reuse object for cases where arrays of some fixed type and size are required by the application over and over
C geotess::CPPUtils | Basic static utility functions and variables
C geotess::CpuTimer | Wall clock and cpu timing information
C geotess::EarthShape | Defines the ellipsoid that is to be used to convert between geocentric and geographic latitude and between depth and radius
C geotess::Edge | Stores information about the connection between two adjacent vertices which separates two neighboring triangles
C geotess::GeoTessData | Abstract base class that manages the data values attached to a single grid point
C geotess::GeoTessDataArray< T > | Manages a 1D array of data values attached to a single grid node
C geotess::GeoTessDataValue< T > | Manages a single data value attached to a grid node
C geotess::GeoTessEnumType | The base class for all "enum" types
C geotess::GeoTessDataType | Enumeration of supported DataType including DOUBLE, FLOAT, LONG, INT, SHORT and BYTE
C geotess::GeoTessInterpolatorType | Enumeration of the interpolation algorithms supported by GeoTess including LINEAR, NATURAL_NEIGHBOR and CUBIC_SPLINE
C geotess::GeoTessOptimizationType | Enumeration of the optimization strategies supported by GeoTess including OptimizationType::SPEED and OptimizationType::MEMORY
C geotess::GeoTessProfileType | Enumeration of the valid Profile types, including EMPTY, THIN, CONSTANT, NPOINT and SURFACE
C geotess::GeoTessException | An exception class for all GeoTess objects
C geotess::GeoTessGreatCircle | Manages information about a great circle path that extends from one point to another point, both or which are located on the surface of a unit sphere
C geotess::GeoTessGrid | Manages the geometry and topology of one or more multi-level triangular tessellations of a unit sphere. Has many functions to retrieve information about the grid but knows nothing about Data
C geotess::GeoTessHorizon | An abstract class that represents a single "surface" within a model
C geotess::GeoTessHorizonDepth | Defines a "surface" in a model that resides at a constant depth
C geotess::GeoTessHorizonLayer | Defines a "surface" in a model that resides at a constant fractional radius within a specified layer
C geotess::GeoTessHorizonRadius | Defines a "surface" in a model that resides at a constant radius
C geotess::GeoTessMetaData | Basic metadata information about a GeoTessModel
C geotess::GeoTessModel | Top level class that manages the GeoTessMetaData, GeoTessGrid and GeoTessData that comprise a 3D Earth model
C geotess::GeoTessModelUtils | A collection of static utilities that extract organized information from a GeoTessModel
C geotess::GeoTessPointMap | Relationships between vertices (2D positions in a tessellation), nodes (1D positions along a radial Profile) and points (3D positions in a model)
C geotess::GeoTessPolygon | An ordered list of points on the surface of a unit sphere that define a closed polygon
C geotess::GeoTessPolygon3D | Extends Polygon by including information and constraints about the radial dimension
C geotess::GeoTessPolygonFactory | Factory method with a static method getPolygon() that returns a pointer to either a Polygon or Polygon3D object
C geotess::GeoTessPosition | Information about an interpolated point at an arbitrary position in a model
C geotess::GeoTessPositionLinear | Implements linear interpolation in geographic dimensions of a grid
C geotess::GeoTessPositionNaturalNeighbor | Implements the Natural Neighbor Interpolation algorithm for the geographic dimensions of the grid
C geotess::GeoTessProfile | Abstract class that manages the radii and data values that span a single layer associated with a single vertex in the model
C geotess::GeoTessProfileConstant | A Profile object that defines two radii at the bottom and top of the associated layer, and a single Data object that represents the model values throughout the layer
C geotess::GeoTessProfileEmpty | A Profile object that defines two radii at the bottom and top of the associated layer, and no Data
C geotess::GeoTessProfileNPoint | A Profile object consisting of N monotonically increasing radii that span the radial extent of a layer, and an equal number of Data objects that define the model values at the corresponding positions
C geotess::GeoTessProfileSurface | A Profile object that defines a single Data object and no radius value
C geotess::GeoTessProfileSurfaceEmpty | A Profile object that defines a single Data object and no radius value
C geotess::GeoTessProfileThin | A Profile object consiting of a single radius value and a single Data object. It represents a profile through a layer that has no thickness
C geotess::GeoTessUtils | Collection of static functions to manipulate geographic information
C geotess::IFStreamAscii | Opens ascii file for read and write access
C geotess::IFStreamBinary | Opens a file for binary read and write access