{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":18,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":128,"n_cols":9,"rows_kept":128,"cut":false,"hidden":false,"merged":[[24,0,24,1],[25,0,26,1],[18,0,18,1],[19,0,19,1],[20,0,20,1],[21,0,21,1],[22,0,22,1],[23,0,23,1],[17,0,17,1],[5,0,5,1],[6,0,6,1],[8,0,8,1],[9,0,9,1],[10,0,10,1],[11,0,11,1],[12,0,12,1],[13,0,13,1],[14,0,14,1],[15,0,15,1],[16,0,16,1]]}
["Program to calculate earth's magnetic field"]
["http://www.ngdc.noaa.gov/geomag-web/#igrfwmm"]
["Latitude: ",null,null,null,"Latitude:35.103821°"]
["Longitude: ",null,null,null,"Longitude:-106.671219°"]
[]
[]
[]
["Latitude: N S","Longitude: E W"]
[]
["Start Date (1900-2015):"]
["  Year:"]
["Month (1-12):"]
["Day (1-31):"]
[]
[]
[]
["End Date (same as starting date for a single day) (1900-2015):"]
["  Year:"]
["Month (1-12):"]
["Day (1-31):"]
[]
[]
[]
["For multiple years, enter step size in years:"]
[]
["Elevation (0-600 km):"]
[]
[]
["  (Results will appear below.)"]
[]
[]
["Results for date: 2012.7896728515625"]
["Declination = 9.018° changing by -0.121 °/year"]
["Inclination = 62.196° changing by -0.023 °/year"]
["X component = 22,940.51 changing by -20.51 nT/year","North"]
["Y component = 3,640.8 changing by -52.92 nT/year","East"]
["Z component = 44,047.34 changing by -96.55 nT/year","Vertical"]
["Horizontal Intensity = 23,227.62 changing by -28.5 nT/year"]
["Total Intensity = 49,796.49 changing by -98.69 nT/year"]
[]
[]
["Reading the results"]
[]
["The magnetic parameters declination, inclination, horizontal component, north component, east component, vertical component, and total field (D, I, H, X, Y, Z, and F) are computed based on the latest International Geomagnetic Reference Field (IGRF) model of the Earth's main magnetic field. Accuracies for the angular components (Declination, D and Inclination, I) are reported in degrees and minutes of arc and are generally within 30 minutes. Accuracies for the force components (Horizontal - H, North - X, East - Y, Vertical - Z, and Total force - F) are generally within 100 to 250 nanotesla. Local disturbances and attempting to use a model beyond its valid date range could cause greater errors. Before using the IGRF please look at the 'Health Warning'. The sign convention used throughout is Declination (D) positive east, Inclination (I) and Vertical intensity (Z) positive down, North component (X) positive north, and East component (Y) positive east. The Horizontal (H) and Total (F) intensities are always positive. For more information on Earth's magnetic field parameters, see our Frequently Asked Questions."]
[]
[]
[]
["Earth Magnetic Field at IBL"]
["Bx=",2.2940000000000001E-5,"T"]
["By=",3.641E-6,"T"]
["Bz=",4.4047E-5,"T"]
[]
["Ion"]
["m=",1,"amu",{"$f":"+B54*1.661E-27","v":1.6610000000000001E-27},"kg"]
["E=",0.1,"MeV",{"$f":"+B55*1000000*1.6E-19","v":1.5999999999999998E-14},"J"]
["q=",1,"e",{"$f":"+B56*1.6E-19","v":1.5999999999999999E-19},"C"]
[]
["beamline"]
["angle (toward north)=",45,"deg",{"$f":"+B59/180*PI()","v":0.78539816339744828},"rad"]
["d (length)=",5.1815999999999995,"m"]
[]
["ion velocity",null,null,"check"]
["V=",{"$f":"SQRT(2*D55/D54)","v":4389248.5358215151},"m/s",{"$f":"SQRT(2*B55/931)*300000000","v":4397050.0803649463}]
["Vx",{"$f":"+SIN(D59)*B63","v":3103667.4039925179},"m/s"]
["Vy",{"$f":"+B63*COS(D59)","v":3103667.4039925183},"m/s"]
["Vz",0,"m/s"]
[]
["Forces"]
["Fx=",{"$f":"+B65*B51-B66*B50","v":136.70723814365846},{"$f":"+B69*$D$56","v":2.1873158102985351E-17},"N"]
["Fy=",{"$f":"+B66*B49-B64*B51","v":-136.70723814365843},{"$f":"+B70*$D$56","v":-2.1873158102985348E-17},"N"]
["Fz=",{"$f":"+B64*B50-B65*B49","v":-59.897677229651606},-9.5836283567442566E-18,"N"]
[]
["flight time"]
["t=",{"$f":"+B60/B63","v":1.1805209838795751E-6},"s"]
[]
["deflection in system coordinate system"]
["X'",{"$f":"0.5*C69*$B$74^2/$D$54","v":9.1761242647897482E-3},"m"]
["Y'",{"$f":"0.5*C70*$B$74^2/$D$54","v":-9.1761242647897465E-3},"m"]
["Z'",-4.0204786293317899E-3,"m"]
[]
["deflection in target coordinate system (assuming target normal to beam)"]
["X\"",{"$f":"+B77*COS(D59)-B78*SIN(D59)","v":1.2976999385286507E-2},"m","left"]
["Z\"",{"$f":"+B79","v":-4.0204786293317899E-3},"m","down"]
[]
["rewritten in a more convenient coordinate system"]
["where x is to right, and z is up"]
["X'''",{"$f":"-B82*1000","v":-12.976999385286508},"mm","right"]
["Z'''",{"$f":"-B83*1000","v":4.02047862933179},"mm","up"]
[]
[]
[null,null,"amu","MeV",null,"deg"]
["Beamline","ion","m","E","q","angle","d(feet)","X'''(mm)","Y'''(mm)"]
["TANDEM     uONE","H",1,1,1,15,10,1.4199610813879002,0.68395401207080064]
[null,"He",4,3,1,15,10,0.40990745628904812,0.19744051649120059]
[null,"C",12,12,4,15,10,0.47332036046263337,0.22798467069026684]
[null,"Si",28,36,5,15,10,0.223622850758496,0.10771263238953618]
[null,"Cu",65,36,5,15,10,0.14677041321412806,7.0695045298688364E-2]
["QASPR3","H",1,1,1,15,8,0.90877509208825646,0.43773056772531238]
[null,"He",4,3,1,15,8,0.26234077202499095,0.12636193055436845]
[null,"C",12,12,4,15,8,0.30292503069608545,0.14591018924177079]
[null,"Si",28,36,5,15,8,0.14311862448543744,6.8936084729303154E-2]
[null,"Cu",65,36,5,15,8,9.3933064457041984E-2,4.524482899116055E-2]
["IBA","H",1,1,1,-15,7,0.69578092988007112,0.3649069862256033]
[null,"He",4,3,1,-15,7,0.2008546535816336,0.10533957336326355]
[null,"C",12,12,4,-15,7,0.23192697662669032,0.1216356620752011]
[null,"Si",28,36,5,-15,7,0.10957519687166299,5.7467448644227294E-2]
[null,"Cu",65,36,5,-15,7,7.1917502474922734E-2,3.7717617655200548E-2]
["QASPR2","H",1,1,1,45,12,2.0447439571985764,0.63354433017815992]
[null,"He",4,3,1,45,12,0.59026673705622945,0.18288849478596086]
[null,"C",12,12,4,45,12,0.68158131906619213,0.21118144339271994]
[null,"Si",28,36,5,45,12,0.32201690509223418,9.9773853701571699E-2]
[null,"Cu",65,36,5,45,12,0.21134939502834435,6.5484585703454917E-2]
["I3TEM","H",1,1,1,90,12,2.0447439571985764,-0.1688988056872944]
[null,"He",4,3,1,90,12,0.59026673705622923,-4.8756885464682848E-2]
[null,"C",12,12,4,90,12,0.68158131906619202,-5.6299601895764786E-2]
[null,"Si",28,36,5,90,12,0.32201690509223413,-2.6599061701452542E-2]
[null,"Cu",65,36,5,90,12,0.21134939502834441,-1.7457765446548208E-2]
[null,"Au",197,5,4,90,12,0.26060383923371455,-2.1526253714622644E-2]
["PELLETRON     uBEAM","H",1,2.5,1,7.5,14,1.7602019927447443,0.88989417757279832]
[null,"3He",3,1,1,7.5,14,1.6068372286530683,0.8123585247485493]
[null,"4He",4,0.75,1,7.5,14,1.6068372286530688,0.81235852474854908]
[null,"C",12,0.25,1,7.5,14,1.6068372286530683,0.8123585247485493]
["HVEE     nanoBEAM","H",1,0.25,1,-15,17,8.2073750504220619,4.3044130211918104]
[null,"P",31,0.25,1,-15,17,1.4740880747780711,0.77309540071913752]
[null,"Sb",121,0.25,1,-15,17,0.7461250045838238,0.39131027465380092]
[null,"H",1,0.02,1,-15,17,29.017452769473618,15.218398181562018]
[null,"P",31,0.02,1,-15,17,5.2116883687089839,2.7333050017631679]
[null,"Sb",121,0.02,1,-15,17,2.6379502517703286,1.383490743778365]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}