# Kuntz

Syntax

  Bc Diffuse For Energy [{of} SpeciesName | {in} MaterialPhaseName | {ls} {a | b | c}] {on} Mesh Extent Name [Touching TouchingMeshExtent | Opposing OpposingMeshExtent] = Kuntz [Using Data Specification Data Spec Name] [Power_Output = power_output | Flux_Output = flux_output | Toggle = toggle | Multiplier = multiplier | File = file | Units = units]

Summary

  Interpolated value from tabulated data for the energy flux. FILE provides the filename for a table which specifies a flux value given X, Y, and Z coordinates and a temperature. UNITS specifies the units the table is in - ENGLISH () or METRIC()

Description

  The following options are present in most boundary conditions/sources. The meaning of each option is as follows:

  Power_Output

    If specified, the total (integrated) power of the given BC/Src is calculated and stored into the global variable name specified as the power_output argument.

  Flux_Output

    If specified, the average flux of the given BC/Src is calculated and stored into the global variable name specified as the flux_output argument.

  Toggle

    If given, specifies which toggle block controls whether this BC is active or not.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
{on} | {@ | at | for | in | on | over} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
power_output | “string” | –
flux_output | “string” | –
toggle | “string” | –
multiplier | real | 1
file | “string” | –
units | “string” | –