# Fluid_Solid_Convection_Coupled_One_Region

Syntax

  Bc Flux For Porous_Enthalpy [{of} SpeciesName | {in} MaterialPhaseName | {ls} {a | b | c}] {on} Mesh Extent Name [Touching TouchingMeshExtent | Opposing OpposingMeshExtent] = Fluid_Solid_Convection_Coupled_One_Region [Using Data Specification Data Spec Name] [Multiplier = multiplier]

Summary

  Boundary condition for loose coupling of enthalpy to a free fluid region

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
{on} | {@ | at | for | in | on | over} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
multiplier | real | 1