# Contact_Resistance

Syntax

  Enforcement For Porous_Enthalpy [{of} SpeciesName | {in} MaterialPhaseName | {ls} {a | b | c}] {=} Contact_Resistance [Opposite_Material_Phase = opposite_material_phase]

Summary

  Applies a contact heat flux of the form to both sides of the contact interface, where is the gap conductance coefficient defined for the surface material.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
{=} | {= | are | is} | –
opposite_material_phase | “string” | –