# Wall_Function

Syntax

  Bc Lumped_Disting For Cvfem_Specific_Dissipation_Rate [{of} SpeciesName | {in} MaterialPhaseName | {ls} {a | b | c}] {@ | at | for | on | over} Mesh Extent Name [Touching TouchingMeshExtent | Opposing OpposingMeshExtent] = Wall_Function [Using Data Specification Data Spec Name] [Wall_Friction_Factor = Wall_Friction_Factor | Wall_Velocity_X = Wall_Velocity_X | Wall_Velocity_Y = Wall_Velocity_Y | Wall_Velocity_Z = Wall_Velocity_Z]

Summary

  CVFEM specific dissipation rate distinguishing condition

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
Wall_Friction_Factor | real | 9.8
Wall_Velocity_X | real | 0
Wall_Velocity_Y | real | 0
Wall_Velocity_Z | real | 0