# Electroosmotic_Velocity

Syntax

  Bc Disting For Momentum [{of} SpeciesName | {in} MaterialPhaseName | {ls} {a | b | c}] {@ | at | for | on | over} Mesh Extent Name [Touching TouchingMeshExtent | Opposing OpposingMeshExtent] = Electroosmotic_Velocity [Using Data Specification Data Spec Name] C = c

Summary

  Electro-osmotic velocity model for momentum distinguishing condition

Description

  This distinguishing condition sets the velocity to simply be a constant multiple of the electric field,

  where is the fluid velocity, is the electric field and is the constant `C` supplied by the user.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
c | real | –