# Porous_Robin_Coupled

Syntax

  Bc Diffuse For Cvfem_Energy [{of} SpeciesName | {in} MaterialPhaseName | {ls} {a | b | c}] {@ | at | for | on | over} Mesh Extent Name [Touching TouchingMeshExtent | Opposing OpposingMeshExtent] = Porous_Robin_Coupled [Using Data Specification Data Spec Name] [Data = data | Enthalpy_Field = enthalpy_field | Enthalpy_Diffusive_Flux_Field = enthalpy_diffusive_flux_field | Averaged_Coeff_Field = averaged_coeff_field]

Summary

  Boundary condition for loose coupling of enthalpy to a porous region

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
data | “string” | –
enthalpy_field | “string” | –
enthalpy_diffusive_flux_field | “string” | –
averaged_coeff_field | “string” | –