# Porous_Robin_Averaged_Coeff

Syntax

  Bc Diffuse For Cvfem_Continuity [{of} SpeciesName | {in} MaterialPhaseName | {ls} {a | b | c}] {@ | at | for | on | over} Mesh Extent Name [Touching TouchingMeshExtent | Opposing OpposingMeshExtent] = Porous_Robin_Averaged_Coeff [Using Data Specification Data Spec Name] [P_Field = P_Field | Massflux_Field = MassFlux_Field | Oppositecoeff_Field = OppositeCoeff_Field]

Summary

  Boundary condition for loose coupling of continuity to a free fluid region

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
P_Field | “string” | –
MassFlux_Field | “string” | –
OppositeCoeff_Field | “string” | –