# 7.6.8.5.1. Aero

Syntax

  Heat Transfer Coefficient [{of} SpeciesName] = Aero [T_On = t_on | T_Off = t_off | Offset_Direction = offset_direction | Coord_Offset = coord_offset | Cone_Length = cone_length | Gas_Constant = gas_constant]

Scope

  Aria Material

Summary

  Heat transfer coefficient for external flow about conical tipped body accounting for flow conditions including Mach number, altitude, fluid properties and local flow regime.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
t_on | real | –
t_off | real | –
offset_direction | “string” | –
coord_offset | “string” | –
cone_length | real | –
gas_constant | real | –