# 7.16.1.43.12. Interfacial_Mass_Transport

Syntax

  Source For Species [{of} SpeciesName | {in} MaterialPhaseName | {ls} {a | b | c}] {@ | at | for | on | over} MeshPartIdentifier = Interfacial_Mass_Transport [Kh = Kh | Gas_Species_Name = gas_species_name | Bnd_Species_Name = bnd_species_name | Multiplier = multiplier | Rmin = Rmin | Nmin = nmin]

Summary

  Liquid-gas interfacial source term associated with bubble mass transfer.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
MeshPartIdentifier | string | –
Kh | real | –
gas_species_name | “string” | –
bnd_species_name | “string” | –
multiplier | real | 1
Rmin | real | 1e-09
nmin | real | 1e-06