# 7.14.1.21. Stress_Tensor_Projection

Syntax

  Eq Stress_Tensor_Projection for Associated DoF [{of} SpeciesName | {in} MaterialPhaseName | {ls} {a | b | c}] {on} MeshPart using Interp with {Term_0} … {Term_N}

Scope

  Aria Region

Summary

  Activates the Stress Tensor Projection equation.

Description

  The only admissible value for Dof is `STRESS_TENSOR`.

  Admissible values of Interp are .

  The only admissible value for Term_n are `DEF`.

  With the exception of `XFER` these terms are described in Generalized Conservation Equation.

  The Meshpart must be an active shell element block.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Associated DoF | string | –
{on} | {@ | at | for | in | on | over} | –
MeshPart | string | –
Interp | string | –
{Term_n} | See Description | –