# Ls_Capillary_Stabilization

Syntax

  Bc Fluxbp For Momentum ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} Mesh Extent Name ([Touching TouchingMeshExtent] | [Opposing OpposingMeshExtent]) = Ls_Capillary_Stabilization [Using Data Specification Data Spec Name] ([Mu0 = mu0] | [Multiplier = multiplier] | [Use_Velocity_Correction = use_velocity_correction])

Summary

  Momentum capillary stabilization flux BP BC using level set normal

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
mu0 | real | 0
multiplier | real | 1
use_velocity_correction | integer | –