# 7.6.18.1.17. User_Plugin

Syntax

  Temperature [{of} SpeciesName] = User_Plugin ([Power_Output = power_output] | [Flux_Output = flux_output] | [Toggle = toggle] | Name = Name | [plugin_parameters])

Scope

  Aria Material

Summary

  Value from a user plugin

Description

  The following options are present in most boundary conditions/sources. The meaning of each option is as follows:

  Power_Output

    If specified, the total (integrated) power of the given BC/Src is calculated and stored into the global variable name specified as the power_output argument.

  Flux_Output

    If specified, the average flux of the given BC/Src is calculated and stored into the global variable name specified as the flux_output argument.

  Toggle

    If given, specifies which toggle block controls whether this BC is active or not.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
power_output | “string” | –
flux_output | “string” | –
toggle | “string” | –
Name | “string” | –
plugin_parameters | “string” | –