# 7.6.2.7.3. Computed_Adiabatic_Wall

Syntax

  Bc Reference Temperature [{of} SpeciesName] = Computed_Adiabatic_Wall (T_On = t_on | T_Off = t_off | Offset_Direction = offset_direction | Coord_Offset = coord_offset | Gas_Constant = gas_constant)

Scope

  Aria Material

Summary

  Adiabatic wall temperature computed based upon freestream and recovery factor.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
t_on | real | –
t_off | real | –
offset_direction | “string” | –
coord_offset | real | –
gas_constant | real | –