# From_Cht_Temperature

Syntax

  Bc Disting For Porous_Enthalpy ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} Mesh Extent Name ([Touching TouchingMeshExtent] | [Opposing OpposingMeshExtent]) = From_Cht_Temperature [Using Data Specification Data Spec Name] (Interface_Name = Interface_Name | Twall_Field = Twall_Field | Tref_Field = Tref_Field | H_Field = H_Field)

Summary

  Porous enthalpy distinguishing condition from conjugate heat transfer temperature

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
Interface_Name | “string” | –
Twall_Field | “string” | –
Tref_Field | “string” | –
H_Field | “string” | –