# 7.17.1.26.24. Pressurization_Model_Venting

Syntax

  Source For Mass Balance ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} MeshPartIdentifier = Pressurization_Model_Venting ()

Summary

  Automatically created source term to apply venting boundary condition to pressurization model bulk node.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
MeshPartIdentifier | string | –