# 7.16.1.22. Nd_Table

Syntax

  Ic For DofName ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} MeshExtent = Nd_Table ([Power_Output = power_output] | [Flux_Output = flux_output] | [Toggle = toggle] | Name = name | [Vars = vars1[ vars2[ vars3[ vars4[ vars5]]]]] | [I0 = i0] | [I1 = i1] | [I2 = i2] | [X = x] | [Y = y] | [Z = z])

Summary

  Value from a multi-dimensional table

Description

  See Multi-dimensional Tables.

  The following options are present in most boundary conditions/sources. The meaning of each option is as follows:

  Power_Output

    If specified, the total (integrated) power of the given BC/Src is calculated and stored into the global variable name specified as the power_output argument.

  Flux_Output

    If specified, the average flux of the given BC/Src is calculated and stored into the global variable name specified as the flux_output argument.

  Toggle

    If given, specifies which toggle block controls whether this BC is active or not.

Parameter | Value | Default
--- | --- | ---
DofName | string | –
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
MeshExtent | string | –
power_output | “string” | –
flux_output | “string” | –
toggle | “string” | –
name | “string” | –
vars | “string”1[ “string”2[ “string”3[ “string”4[ “string”5]]]] | –
i0 | “string” | –
i1 | “string” | –
i2 | “string” | –
x | “string” | –
y | “string” | –
z | “string” | –