# Contact_Resistance_From_Energy

Syntax

  Enforcement For Porous_Enthalpy ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {=} Contact_Resistance_From_Energy ()

Summary

  Applies a contact heat flux of the form to ONLY the side of the contact interface containing a POROUS_ENTHALPY equation, where is the gap conductance coefficient defined for the surface material. Used in conjunction with a CONTACT_RESISTANCE_FROM_POROUS model on energy.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
{=} | {= | are | is} | –