# Open_Adv_Flow

Syntax

  Bc Flux For Cvfem_Level_Set ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} Mesh Extent Name ([Touching TouchingMeshExtent] | [Opposing OpposingMeshExtent]) = Open_Adv_Flow [Using Data Specification Data Spec Name] ([Pressure = pressure] | [Total_Pressure = total_pressure] | Far_Field_Entrainment_Value = far_field_entrainment_value)

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
pressure | real | 0
total_pressure | real | 0
far_field_entrainment_value | real | –