# Conductance

Syntax

  Enforcement For Energy ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {=} Conductance [Toggle = toggle]

Summary

  Applies a contact heat flux of the form to sides and of the contact interface where is a user specified conductance coefficient. Used in conjunction with a CONDUCTANCE COEFFICIENT model.

Description

  The following options are present in most boundary conditions/sources. The meaning of each option is as follows:

  Toggle

    If given, specifies which toggle block controls whether this BC is active or not.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
{=} | {= | are | is} | –
toggle | “string” | –