# Mass_Fluid_Robin_Coupled

Syntax

  Bc Lumped_Flux For Mass_Balance ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} Mesh Extent Name ([Touching TouchingMeshExtent] | [Opposing OpposingMeshExtent]) = Mass_Fluid_Robin_Coupled [Using Data Specification Data Spec Name] ([Coeff_Scaling = coeff_scaling] | P_Field = P_Field | Massflux_Field = MassFlux_Field)

Summary

  Boundary condition for loose coupling of continuity to a free fluid region

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
coeff_scaling | real | 0.001
P_Field | “string” | –
MassFlux_Field | “string” | –