# Tied_Scalar

Syntax

  Bc Interface_Colloc_Disting For Energy ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} Mesh Extent Name ([Touching TouchingMeshExtent] | [Opposing OpposingMeshExtent]) = Tied_Scalar [Using Data Specification Data Spec Name] ([Current_Expr = current_expr] | [Matched_Flux = matched_flux] | [Opposite_Expr = opposite_expr])

Summary

  TIED_SCALAR for energy interface model

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
current_expr | “string” | –
matched_flux | “string” | –
opposite_expr | “string” | –