# Simple_Inflow

Syntax

  Bc Flux For Cvfem_Dispersed_Continuity ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} Mesh Extent Name ([Touching TouchingMeshExtent] | [Opposing OpposingMeshExtent]) = Simple_Inflow [Using Data Specification Data Spec Name] ([Velocity_X = Velocity_X] | [Velocity_Y = Velocity_Y] | [Velocity_Z = Velocity_Z])

Summary

  Inflow mass flux for dispersed continuity equation; specified density and velocity

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
Data Spec Name | string | –
Velocity_X | real | 0
Velocity_Y | real | 0
Velocity_Z | real | 0