# 7.17.1.27.5. Electrode_Object_Old

Syntax

  Source For Mass Balance ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} MeshPartIdentifier = Electrode_Object_Old (F = f | Electrodefile = electrodeFile | Kmolconversion = kmolConversion | [Jconversion = JConversion] | [Meterconversion = meterConversion] | [Max_Sub_Timesteps = max_sub_timesteps] | [Base_Delta = base_delta])

Summary

  Electrode object source for current equation to be used with porous electrodes

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
MeshPartIdentifier | string | –
f | real | –
electrodeFile | “string” | –
kmolConversion | real | –
JConversion | real | 1
meterConversion | real | 1
max_sub_timesteps | integer | 100
base_delta | real | 1e-05