# Porous_Robin_Coupled_With_Solid_Phase_Convection_One_Region

Syntax

  Bc Flux For Cvfem_Energy ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} Mesh Extent Name ([Touching TouchingMeshExtent] | [Opposing OpposingMeshExtent]) = Porous_Robin_Coupled_With_Solid_Phase_Convection_One_Region ([Data = data] | [Multiplier = multiplier])

Summary

  Boundary condition for coupling of enthalpy to a porous region in the same region.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
Mesh Extent Name | string | –
TouchingMeshExtent | string | –
OpposingMeshExtent | string | –
data | “string” | –
multiplier | real | 1