# 7.17.1.21.39. Lumped_Polynomial

Syntax

  Source For Energy ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {@ | at | for | on | over} MeshPartIdentifier = Lumped_Polynomial ([Power_Output = power_output] | [Toggle = toggle] | Variable = variable | Order = order | [Variable_Offset = variable_offset] | [C0 = c0] | [C1 = c1] | [C2 = c2] | [C3 = c3] | [C4 = c4] | [C5 = c5] | [C6 = c6] | [C7 = c7] | [C8 = c8])

Summary

  Value from a polynomial function

Description

  The following options are present in most boundary conditions/sources. The meaning of each option is as follows:

  Power_Output

    If specified, the total (integrated) power of the given BC/Src is calculated and stored into the global variable name specified as the power_output argument.

  Toggle

    If given, specifies which toggle block controls whether this BC is active or not.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
MeshPartIdentifier | string | –
power_output | “string” | –
toggle | “string” | –
variable | “string” | –
order | integer | –
variable_offset | real | 0
c0 | real | 0
c1 | real | 0
c2 | real | 0
c3 | real | 0
c4 | real | 0
c5 | real | 0
c6 | real | 0
c7 | real | 0
c8 | real | 0