# Shell_Enclosure

Syntax

  Enforcement For Porous_Enthalpy ([{of} SpeciesName] | [{in} MaterialPhaseName] | [{ls} {a | b | c}]) {=} Shell_Enclosure (Enclosure = enclosure | [Toggle = toggle])

Summary

  Applies a contact heat flux copied from the radiative flux field populated by Chaparral during an enclosure radiation solve. The flux field is interpolated from the contact surface to the current surface. Temperature coupling with the current surface temperature is also implemented using the method specified in the enclosure definition. The only parameter required is the name of the enclosure definition to couple with.

Description

  The following options are present in most boundary conditions/sources. The meaning of each option is as follows:

  Toggle

    If given, specifies which toggle block controls whether this BC is active or not.

Parameter | Value | Default
--- | --- | ---
{of} | {of | species | subindex} | –
SpeciesName | string | –
{in} | {in | material_phase} | –
MaterialPhaseName | string | –
{ls} | {levelset_phase | ls} | –
{=} | {= | are | is} | –
enclosure | “string” | –
toggle | “string” | –